[Version]
Signature="$CHICAGO$"
Class=USB
provider=%ProviderName%
LayoutFile=layout.inf
DriverVer=06/12/2002, 1.0.0.0

[Manufacturer]
%MfgName%=Casio

[Casio]
%DevName%=PVUSB, USB\VID_07CF&PID_6101

[PreCopySection]
HKR,,NoSetupUI,,1

[DestinationDirs]
PVUSB.Files = 10,System32\Drivers

[PVUSB]
CopyFiles=PVUSB.Files
AddReg=PVUSB.AddReg

[PVUSB.HW]
AddReg=PVUSB.AddReg.HW

[PVUSB.NT]
;CopyFiles=PVUSB.Files
;AddReg=PVUSB.NT.AddReg -- No AddReg needed for W2K

[PVUSB.NT.Services]
AddService = PVUSB, 0x00000002, PVUsbService_Inst


[PVUSB.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,CESG502.sys
HKR,,"DebugLevel",0x10001,2

[PVUSB.AddReg.HW]
HKR,,"DEV_GUID",,{CDE970E0-E265-11d5-8E17-0000C0CBB2F3}
;HKR,,"DebugLevel",0x10001,2
;HKR,,"MaximumTransferSize",0x10001,4096


[PVUSB.NT.AddReg]

[PVUsbService_Inst]
DisplayName    = %SvcName%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 0               ; SERVICE_ERROR_IGNORE
ServiceBinary  = %12%\CESG502.sys
LoadOrderGroup = Extended base

[PVUSB.Files]
CESG502.sys

[SourceDisksNames.x86]
1 = %DiskId1%,,,""

[SourceDisksFiles]
CESG502.sys = 1,,

;---------------------------------------------------------------;

[Strings]
ProviderName="HSDS"
MfgName="CASIO COMPUTER CO.,LTD."
DevName="CESG502 USB"
SvcName = "CESG502 USB Driver"
DiskId1 = "CESG502 Driver Disk"
